APPROACH: The task involved configuring VLANs, IP addresses, and MAC addresses on switches, enabling specific interfaces, and setting up PC IP addresses accordingly.

SOLUTION:

1. First do the configurations on senior switch:

* en mode
* config mode
* interface vlan1
* ip address<vlan1 ip> <subnet mask>
* mac-address <mac address>
* no shutdown
* exit
* exit

1. Repeat same steps on all the switches.