Approach: The problem involved establishing connectivity between PCs connected to two switches within the same VLAN. Key considerations included configuring the switches to ensure proper VLAN assignment and enabling communication between the PCs.

Solution:

1. Checking the connectivity between network and CAM table using show mac-address-table
2. Switch’s mac address is listed in table
3. Generate traffic by ping another device IP address command to get the IP address and MAC address