APPROACH:  The problem involved configuring VLANs and enabling SSH on the Admin and Senior switches. It required analyzing VLAN configurations, setting up ports accordingly, and enabling SSH access.

Solution:

1. Check the connectivity of network
2. Go to enable mode
3. Check VLAN interface using **show vlan** command
4. Check IP address interface by using **show ip address** command