APPROACH: The problem involves accessing the configurations of two switches, Senior Switch and Admin Switch, which are likely protected by passwords. The objective is to reveal the passwords configured for both switches and any relevant interface configurations

SOLUTION:

1. Configuring timeout by using following commands :

* In config mode **line con 0**
* Configuring VTY line 0 through 4- **line vty 0 4**
* Setting inactivity timeout – **exec-timeout 6 30**
* exit
* To save configuration – **write memory** in en mode