**Albus Security**

**Practical Challenge – 1**

**Approach:** To solve the task, I will review the Vlan configuration and Vlan Trunk Configuration.

**Solution:**

Admin Switch **-**

* **configure terminal**
* **interface Gig0/1**
* **switchport mode trunk**
* **switchport trunk allowed vlan 1-1005**
* Same configuration for **Gig0/2**

Senior Switch –

* **configure terminal**
* **interface Gig0/1**
* **switchport mode trunk**
* **switchport trunk allowed vlan 1-1005**
* Same configuration for **Gig0/2**

Junior Switch –

* **configure terminal**
* **interface Gig0/1**
* **switchport mode trunk**
* **switchport trunk allowed vlan 1-1005**
* Same configuration for **Gig0/2**

Fresher Switch –

* **configure terminal**
* **interface Gig0/1**
* **switchport mode trunk**
* **switchport trunk allowed vlan 1-1005**
* Same configuration for **Gig0/2**