**Albus Security**

**Practical Challenge – 2**

**Approach:** To solve the task, I will review the Vlan configuration.

**Solution:**

Admin Switch **-**

1. Access the Switch CLI: **en**

2. Enter Global Configuration Mode: **configure terminal**

3. Select the Trunk Interface: **interface fa0/1**

4. Limit VLANs on the Trunk: **switchport trunk allowed vlan 1,20**

5. Changing Mode: **switchport mode dynamic desirable**

Senior Switch **-**

1. Access the Switch CLI: **en**

2. Enter Global Configuration Mode: **configure terminal**

3. Select the Trunk Interface: **interface fa0/1**

5. Allow interfaces: **switchport access vlan 20**

5. Changing Mode: **switchport mode dynamic desirable**

6. Select interface: **interface fa0/3**

7. Changing vlan: **switchport access vlan 20**