**Albus Security**

**Practical Challenge – 5**

**Approach:** To solve the task, I will review the Spanning tree configuration.

**Solution:**

Senior Switch: -

* **conf t**
* **spanning-tree mode rapid-pvst**
* **int fa0/3**
* **switchport mode trunk**
* **switchport trunk allowed vlan add 1**
* **show spanning-tree**

Junior Switch: -

* **conf t**
* **spanning-tree mode rapid-pvst**
* **int fa0/1**
* **switchport mode trunk**
* **switchport trunk allowed vlan add 2**
* **int fa0/1**
* **switchport mode trunk**
* **switchport trunk allowed vlan add 2**
* **int fa0/1**
* **switchport mode trunk**
* **switchport trunk allowed vlan add 2**